품 명		POWER AMPLIFIER
모 델		CPD2600	제조사	Wharfedale
Technical Specifications
	Stereo Power Output - 8 ohms*2 : 650W - 4 ohms*2 : 1000W Bridged Mono Output - 8 ohms : 1940W Frequency Response - +/-1dB @ 8 Ohmes : 20Hz-20KHz - +/-3dB @ 8 Ohmes : 20Hz-30KHz Topology : Class H Connectors - Signal Input and Output : Female and Male XLR Jacks - Power Output : SPEAKON Jacks AC Power Options : AC110-120V~ 50/60Hz or AC100V~ 50/60Hz; AC220-230V~ 50/60Hz or AC240V~ 50/60Hz Dimensions : 88 x 483 x 450 mm Weight (Net) : 19 kg

*) POWER AMPLIFIER

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 2채널 파워 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1000W*2@4Ohms (RMS)

650W*2@8Ohms (RMS)

2 channels XLR inputs with link outputs

3 operation modes (PARALLEL, STEREO and BRIDGE)

Power, Protect, Signal and Limiter indicators

Thermal protect, over current protect, DC protect, output short protect, power on/off mute

Ultra quiet variable speed fans

Speakon outputs for speakers

2U rack mount chassis

3. 규격 및 사양

Stereo Power Output

- 8 ohms*2	: 650W

- 4 ohms*2	: 1000W

Bridged Mono Output

- 8 ohms	: 1940W

Sensitivity	: 0dBu (0.775Vrms)

Balanced XLR input	: 20Kohms

Maximum Input Level	: 22dBu (9.7Vrms)

Voltage Gain	: 39dB

Slew Rate	: >40V / us

Crosstalk	: <-70dB

S/N	: >100dB

Distortion (1W)	: <0.02%

Frequency Response

- +/-1dB @ 8 Ohmes	: 20Hz-20KHz

- +/-3dB @ 8 Ohmes	: 20Hz-30KHz

Damping Factor	: >300

Topology	: Class H

Connectors

- Signal Input and Output	: Female and Male XLR Jacks

- Power Output	: SPEAKON Jacks

Controls

- Front panel	: AC Switch, CH 1 and CH 2 Gain Knobs

- Rear panel	: Parallel, Stereo & Bridge Mode Switch; Limiter Switch

Protections	: Thermal protect, Over-current protect, Output DC	protect, Output short protect, Power on/off mute

Indictors	: Power, Protect, Signal, Limiter

Cooling	: Variable Speed Fan

AC Power Options	: AC110-120V~ 50/60Hz or AC100V~ 50/60Hz;

AC220-230V~ 50/60Hz or AC240V~ 50/60Hz

Dimensions	: 88 x 483 x 450 mm

Weight (Net)	: 19 kg

* CPD2600 동급이상품.