품 명		PASSIVE PA SPEAKER
모 델		DELTA X15	제조사	Wharfedale
Technical Specifications
	System Type : Passive Frequency Response (+/-3dB) : 50Hz-20kHz Frequency Range (-10dB) : 45Hz-20kHz Sensitivity (2.83v/1m) : 98dB Calculated Maximum SPL @1m : 131dB System Rated Impedance : 8Ω Low Frequency Transducer - Size : 404mm / 15" Paper - Voice Coil Size : 77.1mm / 3" - Rated Impedance : 8Ω High Frequency Transducer - HF Driver Type : Compression Driver - Voice Coil Size : 50.8mm / 2" Titanium - Exit Size : 35.6mm / 1.4" - Rated Impedance : 8Ω - Nominal Coverage (HxV) : 90° x 45° Power - System Power (Cont./Prg./Peak) : 500W / 1000W / 2000W Dimensions (H x W-Front / W-Rear x D) : 700 x 446/281.4 x 406 mm Weight : 29.9 kg

*) PASSIVE PA SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 라우드 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

High power, low distortion cast frame woofers

1.4" exit, 2" titanium diaphragm compression drivers

Externally switchable full range/bi-amp operation

90°x45° elliptical waveguides

Dual angle pole mount receptacles

Plywood construction with internal bracing

4-way high impact plastic carry handles

Rhino Rock texturised composite finish

Parallel speakon compatible inputs

3. 규격 및 사양

System Type	: Passive

Configuration	: Two-way

Frequency Response (+/-3dB)	: 50Hz-20kHz

Frequency Range (-10dB)	: 45Hz-20kHz

Sensitivity (2.83v/1m)	: 98dB

Calculated Maximum SPL @1m	: 131dB

System Rated Impedance	: 8Ω

Low Frequency Transducer

- Size	: 404mm / 15" Paper

- Voice Coil Size	: 77.1mm / 3"

- Rated Impedance	: 8Ω

- LF Power	(re:AES2-2012)	: 500W

High Frequency Transducer

- HF Driver Type	: Compression Driver

- Voice Coil Size	: 50.8mm / 2" Titanium

- Exit Size	: 35.6mm / 1.4"

- Diaphragm Material	: Titanium

- Rated Impedance	: 8Ω

- HF Power (re:AES2-2012)	: 50W

- Nominal Coverage (HxV)	: 90° x 45°

Power

- System Continuous Power	: 500W

- System Programme Power	: 1000W

- System Peak Power	: 2000W

- Crossover frequency	: 1.8kHz

- Input Connector	: 2 x NL4 (speakON Compatible)

Hardware

- Pole Mount	: Dual Angle (0° / 10° ) 35mm Socket

- Handles	: 2 on Sides

- Rigging points	: 6 x M10

- Enclosure Material	: 15mm Plywood

- Grille Material	: 1.5 mm Steel

Dimensions (H x W-Front / W-Rear x D) : 700 x 446/281.4 x 406 mm

Weight	: 29.9 kg

* DELTA X15 동급이상품.