품 명		FIXED I/O BOX
모 델		DL32	제조사	MIDAS
Technical Specifications
	32 award-winning MIDAS PRO microphone preamplifi ers with switchable 48 V phantom power 16 electronically balanced low impedance line level outputs ULTRANET personal monitoring system connectivity for in-ear applications Digital audio and control connectivity for TURBOSOUND speaker systems with ULTRANET networking capability Dual AES50 SuperMAC ports for cascading additional DL16 stageboxes—no merger or router required Automatic AES50 stage-split mode when connected between MIDAS M32 Series FOH and monitor consoles Dual ADAT outputs providing 16-channel digital output on two optical TOSLINK* connectors 2 AES-3 ports (AES/EBU), for directly connecting PA system controllers with digital inputs Remote operation via shielded CAT5e cable up to 330 ft / 100 m length Mute All function for quietly patching any inputs on stage MIDI In/Out for bidirectional communication between MIDAS M32 Series console and on-stage MIDI devices Features Neutrik etherCON* AES50 and ULTRANET network ports Rugged 3U rackmount chassis for durability in portable applications Input : 32 ch Output : 16 ch AES50 : A,B ULTRANET : 1ch MIDI : In,Out Dim : 483 x 138 x 242 mm

*) FIXED I/O BOX

1. 개요

본 기기는 Main Digital Mixer와 연동하여 사용가능한 Stage Box이다.

2. 기능 및 특성

32 award-winning MIDAS PRO microphone preamplifi ers with switchable 48 V phantom power

16 electronically balanced low impedance line level outputs

ULTRANET personal monitoring system connectivity for in-ear applications

Digital audio and control connectivity for TURBOSOUND speaker systems with ULTRANET networking capability

Dual AES50 SuperMAC ports for cascading additional DL16 stageboxes—no merger or router required

Automatic AES50 stage-split mode when connected between MIDAS M32 Series FOH and monitor consoles

Dual ADAT outputs providing 16-channel digital output on two optical TOSLINK* connectors

2 AES-3 ports (AES/EBU), for directly connecting PA system controllers with digital inputs

Remote operation via shielded CAT5e cable up to 330 ft / 100 m length

Mute All function for quietly patching any inputs on stage

MIDI In/Out for bidirectional communication between MIDAS M32 Series console and on-stage MIDI devices

Features Neutrik etherCON* AES50 and ULTRANET network ports

Rugged 3U rackmount chassis for durability in portable applications

3. 규격 및 사양

Input	: 32 ch

Output	: 16 ch

AES50	: A,B

ULTRANET	: 1ch

MIDI	: In,Out

Dim	: 483 x 138 x 242 mm

* DL32 동등이상품.