품 명		DYNAMIC MIC.
모 델		DM5.0S	제조사	Wharfedale
Technical Specifications
	Transducer Type : Dynamic Frequency Response : 50Hz-12kHz Polar Pattern : Unidirectional Output Impedance : 600ohms Sensitivity : -51dB (0dB=1V/Oa) Off axis rejection : >20dB at 180° Maximum SPL : >135dB Cable/Connector : 3 pin gold plated male XLR Polarity : Positive voltage on pin 2 relative to pin 3 of output XLR connector Housing : Zinc alloy Weight : 300 g

*) DYNAMIC MIC

1. 개요

본 기기는 다이나믹 핸드타입 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Live dynamic microphone

Supercardioid polar pattern

High performance capsule

Tailored for vocals

Steel mesh grille

Available with on/off switch

3. 규격 및 사양

Transducer Type	: Dynamic

Frequency Response	: 50Hz-12kHz

Polar Pattern	: Unidirectional

Output Impedance	: 600ohms

Sensitivity	: -51dB (0dB=1V/Oa)

Off axis rejection	: >20dB at 180°

Maximum SPL	: >135dB

Cable/Connector	: 3 pin gold plated male XLR

Polarity	: Positive voltage on pin 2 relative to pin 3 of	output XLR connector

Housing	: Zinc alloy

Weight	: 300 g

* DM5.0S 동급이상품.