품 명		MIXING CONSOLE
모 델		L-PAD 12CX	제조사	RCF AUDIO
Technical Specifications
	Mono channels Microphone input : XLR balanced Frequency response : 20Hz to 22KHz,+/-1dB Gain range : 0dB to -50dB Line input : 1/4’ TRS balanced Frequency response : 20Hz to 22kHz,+/-1dB Sensitivity range : +15dB~ -35dB Stereo input channels Mic input : XLR balanced Line input : 1/4’ TRS or TRS/RCA un-balanced Frequency response : 20Hz to 22kHz,+/-1dB Sensitivity range : +15dBu~ -35dBu Channels EQ Mono channel Stereo channel High : +/-15dB @12kHz : +/-15dB @12kHz Mid : +/-15dB @2.5kHz Low : +/-15dB @80Hz : +/-15dB @80Hz DSP section A/D and D/A converters : 24bit Type of effects : Echo ,Echo+Verb , Tremolo , Plate , Chorus ,Vocal Rotary , Small Room , Flange + Verb , Large Hall Controls : 100 position preset selector(10 preset x 10 variation) Main mix section Max. MAIN MIX output : +22dBu XLR balanced (+16dBu un-balanced) AUX range : OFF to +15dB Fader range : OFF to +10dB PHONES/CONTROL-ROOM range : OFF to +15dB Power supply Main voltage : 100-240VAC ~ 50/60Hz Power consumption : 40W max Dimensions : 480 mm x 340 mm x 100 mm (L x W x H) Weight : 3.85 kg

*) 12 CHANNEL MIXING CONSOLE

1. 개요

본 기기는 소리 방향 설정, 소리 크기 변경, 소리 신호의 음색 및 세기를 제어하는 오디오 믹서이다.

2. 기능 및 특성

6 mono INPUT + 4 stereo INPUT

4 Compressors (Ch. 1-4)

3band/2band EQ

1 AUX send

1 FX send

Internal Digital Effects: 99 preset

Internal PSU 100V-240V, 50-60Hz, 40W

3. 규격 및 사양

Mono channels

Microphone input	: XLR balanced

Frequency response	: 20Hz to 22KHz,+/-1dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Gain range	: 0dB to -50dB

Max. input	: +15 dB (balanced)

SNR	: <-100dBr A-weighted

Phantom power	: +48V with switch control

Line input	: 1/4’ TRS balanced

Frequency response	: 20Hz to 22kHz,+/-1dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Sensitivity range	: +15dB~ -35dB

Compressor	: GAIN: 0 ---> 9dB | THRESHOLD: 20dB --->	5dB

Stereo input channels

Mic input	: XLR balanced

LOW CUT	: 75Hz

Line input	: 1/4’ TRS or TRS/RCA un-balanced

Frequency response	: 20Hz to 22kHz,+/-1dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Sensitivity range	: +15dBu~ -35dBu

SNR	: <-100dBr A-weighted

Channels EQ	Mono channel	Stereo channel

High	: +/-15dB @12kHz	: +/-15dB @12kHz

Mid	: +/-15dB @2.5kHz

Low	: +/-15dB @80Hz	: +/-15dB @80Hz

2-TRACK IN

TAPE IN	: RCA jack

Frequency Response	: 20Hz to 22kHz,+/-1dB

Distortion (THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Gain Range	: OFF to 15dB

STEREO RETURN

Input	: 1/4’ TRS un-balanced

Frequency response	: 20Hz to 22kHz,+/-1dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

GAIN range	: OFF TO +15dB

SNR	: <-100dBr A-weighted

Impedances

Microphone input	: 1.8kΩ

All other input	: 10kΩ or greater

Tape out	: 1kΩ

All other out	: 120Ω

DSP section

A/D and D/A converters	: 24bit

Type of effects	: Echo ,Echo+Verb , Tremolo , Plate , Chorus	,Vocal Rotary , Small Room , Flange + Verb ,	Large Hall

Controls	: 100 position preset selector(10 preset x 10	variation)

FOOT-SW	: Mute switch & Foot-switching with LED indicator

TIP:FX SLEEVE:GND

Main mix section

Max. MAIN MIX output	: +22dBu XLR balanced (+16dBu un-balanced)

AUX range	: OFF to +15dB

Fader range	: OFF to +10dB

PHONES/CONTROL-ROOM range	: OFF to +15dB

Hum & Noise	: <-80dB @ 20Hz~22kHz A-weighted 1 channel &	MAIN level:0dB,the other :minimum

Crosstalk	: <-80dB @0dB 20Hz~22kHz A-weighted MAIN

level:0dB,the other :minimum

Power supply

Main voltage	: 100-240VAC ~ 50/60Hz

Fuse	: T1.6AL AC250V

Power consumption	: 40W max

Dimensions	: 480 mm x 340 mm x 100 mm (L x W x H)

Weight	: 3.85 kg

* L-PAD 12CX 동등이상품.