품 명		MIXING CONSOLE
모 델		L-PAD 6	제조사	RCF AUDIO
Technical Specifications
	Mono channels Microphone input : XLR balanced Frequency response : 10Hz to 55KHz,+/-3dB Gain range : 0dB to -50dB Line input : 1/4’ TRS with balanced Frequency response : 10Hz to 55kHz,+/-3dB Sensitivity range : +15dB~ -35dB Stereo input channels Line input : 1/4’ TRS with un-balanced Frequency response : 10Hz to 55kHz,+/-3dB Sensitivity range : +22dBu Channels EQ Mono channel Stereo channel High : +/-15dB @12kHz : +/-15dB @12kHz Mid : +/-15dB @2.5kHz Low : +/-15dB @80Hz : +/-15dB @80Hz Main mix section Max. MAIN MIX output : +22dBu un-balanced AUX range : OFF to +10dB Fader range : OFF to +10dB PHONES/CONTROL-ROOM range : OFF to +10dB Power supply AC adaptor 18VAC : 1000mA Power consumption : 17W (all loaded) Dimensions : 275mm x 195 mm x 75 mm (L x W x H) Weight : 1.3 kg

*) 6 CHANNEL MIXING CONSOLE

1. 개요

본 기기는 소리 방향 설정, 소리 크기 변경, 소리 신호의 음색 및 세기를 제어하는 오디오 믹서이다.

2. 기능 및 특성

2 mono INPUT + 2 stereo INPUT

1 AUX send

3band/2band EQ

External PSU 18V~ 1000mA

3. 규격 및 사양

Mono channels

Microphone input	: XLR balanced

Frequency response	: 10Hz to 55KHz,+/-3dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Gain range	: 0dB to -50dB

Max. input	: +15 dB

SNR	: <-100dBr A-weighted

Phantom power	: +48V with switch control

Line input	: 1/4’ TRS with balanced

Frequency response	: 10Hz to 55kHz,+/-3dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Sensitivity range	: +15dB~ -35dB

Stereo input channels

Line input	: 1/4’ TRS with un-balanced

Frequency response	: 10Hz to 55kHz,+/-3dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Sensitivity range	: +22dBu

SNR	: <-100dBr A-weighted

Channels EQ	Mono channel	Stereo channel

High	: +/-15dB @12kHz	: +/-15dB @12kHz

Mid	: +/-15dB @2.5kHz

Low	: +/-15dB @80Hz	: +/-15dB @80Hz

2-TRACK IN

TAPE IN	: RCA jack

Frequency Response	: 10Hz to 55kHz,+/-3dB

Distortion (THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

Gain Range	: OFF to +10dB

STEREO RETURN

Input	: 1/4’ TRS with un-balanced

Frequency response	: 10Hz to 55kHz,+/-3dB

Distortion(THD+N)	: <0.03% at +0dB ,22Hz~22kHz A-weighted

GAIN range	: OFF TO +10dB

SNR	: <-100dBr A-weighted

Impedances

Microphone input	: 3.6kΩ

All other input	: 10kΩ or greater

Tape out	: 1kΩ

All other out	: 120Ω

Main mix section

Max. MAIN MIX output	: +22dBu un balanced

AUX range	: OFF to +10dB

Fader range	: OFF to +10dB

PHONES/CONTROL-ROOM range	: OFF to +10dB

Hum & Noise	: <-80dB @ 20Hz~22kHz A-weighted 1 channel &	MAIN level:0dB,the other :minimum

Crosstalk	: <-80dB @0dB 20Hz~22kHz A-weighted MAIN

level:0dB,the other :minimum

Power supply

AC adaptor 18VAX	: 1000mA

Power consumption	: 17W (all loaded)

Dimensions	: 275 mm x 195 mm x 75 mm (L x W x H)

Weight	: 1.3kg

* L-PAD 6 동등이상품.