품 명		ACTIVE PA SPEAKER
모 델		PSX115	제조사	Wharfedale
Technical Specifications
	System Type : Active 15" 2-way Bi-Amplified system Frequency Response (+/-3dB) : 50Hz-20kHz Sensitivity @ 1W / 1m : 97dB Maximum SPL (peak @1m) : 130dB Low Frequency Transducer - Size : 381mm / 15" - Coil Size : 50.8mm / 2.0" - Impedance : 4Ω High Frequency Transducer - Type : Compression Driver - Coil Size : 44.5mm / 1.75" - Exit Size : 25mm / 1" - Impedance : 8Ω - High Frequency Coverage (HxV) : 90° x 60° Amplifiers - Low-Frequency Power Amplifier (Class D) : 350w Continuous / 700w Peak - High- Frequency Power Amplifier (Class AB ) : 100w Continuous / 200w Peak Dimensions (H x W-Front/W-Rear x D) : 603 x 455/262 x 401.8 mm Weight : 19.2 kg

*) ACTIVE PA SPEAKER

1. 개요

본 기기는 앰프가 내장된 2-way 라우드 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Bi-amplified with high power output

Easy operation

Portable and durable

1.75" HF compression driver

Convection cooling

4 x M8 rigging points

3. 규격 및 사양

System Type	: Active 15" 2-way Bi-Amplified system

Frequency Response (+/-3dB)	: 50Hz-20kHz

Sensitivity @ 1W / 1m	: 97dB

Maximum SPL (peak @1m)	: 130dB

Low Frequency Transducer

- Size	: 381mm / 15"

- Coil Size	: 50.8mm / 2.0"

- Impedance	: 4Ω

High Frequency Transducer

- Type	: Compression Driver

- Coil Size	: 44.5mm / 1.75"

- Exit Size	: 25mm / 1"

- Diaphragm Material	: Titanium

- Impedance	: 8Ω

- High Frequency Coverage (HxV)	: 90° x 60°

Amplifiers

- Low-Frequency Power Amplifier (Class D)

: 350w Continuous / 700w Peak

- High- Frequency Power Amplifier (Class AB )

: 100w Continuous / 200w Peak

Crossover Frequency	: HI PASS 2.4kHz LOW PASS 2.4kHz

Equalization	: +/-12dB Gain for bass and treble

Amplifier Protection

- Power On Protection	: Power switch on / off mute

- Thermal Protection	: Amplifier shutdown, auto reset

- Driver, DC and Short Protection	: Yes

- Input type	: Balanced

- Input Connectors	: TRS JACK AND FEMALE XLR

- Input Impedance	: 47KΩ Balanced

- Maximum Input Level	: 5V

- Line Input Sensitivity	: -10dB

- Mic Input Sensitivity	: -40dB

- Line Output Connector	: MALE XLR

AC Power details

- Power Supply	: SMPS

- AC Power Options	: 100V-120V and 200V-240V

Rigging / Bracket / Mounting Options : 4 x M8

35mm Pole-mount with lock screw

3 carry handles (one on each side, one on top)

Optional wall-mount bracket

Enclosure

- Enclosure Material	: Injection Moulded Polypropylene

- Grille	: 1.2mm steel

Dimensions (H x W-Front/W-Rear x D) : 603 x 455/262 x 401.8 mm

Weight	: 19.2 kg

* PSX115 동급이상품.