품 명		LINE ARRAY SPEAKER
모 델		WLA-25	제조사	Wharfedale
Technical Specifications
	System Type : Passive Configuration : two-way Frequency Response (+/-3dB) : 108Hz - 18kHz Frequency Range (-10dB) : 108Hz - 20kHz Calculated Maximum SPL @1m : HF:135dB/LF:127dB System Rated Impedance : 16Ω Low Frequency Transducer - Size : 130mm / 5" - Coil Size : 35.0mm / 1.4" - LF Power re:AES2-2012 : 2X60W High Frequency Transducer - HF Driver Type : Compression Driver - Coil Size : 44mm / 1.75" - Exit Size : 1" - HF Power re:AES2-2012 : 40W - Waveguide Type : square - Nominal Coverage (HxV) : 100°x10° Power - System Continuous Power : HF:40W/LF:120W - System Programme Power : HF:80W/LF:240W - System Peak Power : HF:160W/LF:480W Dimensions (HxWxD) : 536 x 363 x 164 mm Net Weight : 13 kg

*) LINE ARRAY SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 라인어레이 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

High sensitivity, Full Horn Loaded design

120W RMS/240W Program/480W Peak Power Handling

Dual 5" woofer, 1.5" voice coils

1x1" exit HF compression driver

1.7" Titanium diaphragm, neodymium magnet compression driver

100°x10° degree constant-directivity horn

Nominal Passive Crossover Network

Front hinged rigging system

Captive rigging hardware with tethered quick release pins

Comprehensive adjustable splay angles

Integral, side plate adjustable rigging system, vertical splay adjustable in 1° increments from 0°-10°

Trapezoid Baltic birch plywood enclosure

2 x Parallel Speakon Inputs

Constant directivity waveguides

3. 규격 및 사양

System Type	: Passive

Configuration	: two-way

Frequency Response (+/-3dB)	: 108Hz - 18kHz

Frequency Range (-10 dB)	: 108Hz - 20kHz

Sensitivity (2.83v/1m)	: HF:108dB/LF:100dB

Calculated Maximum SPL @1m	: HF:135dB/LF:127dB

System Rated Impedance	: 16Ω

Low Frequency Transducer

- LF Size	: 130mm / 5"

- LF Voice-Coil Size	: 35.0mm / 1.4"

- LF Magnet Material	: ferrite

- LF Frame Material	: aluminium

- Rated Impedance	: 16Ω

- LF Power re:AES2-2012	: 2X60W

High Frequency Transducer

- HF Driver Type	: Compression Driver

- Coil Size	: 44mm / 1.75"

- Exit Size	: 1"

- HF Magnet Material	: NdFeB

- Diaphragm Material	: Titanium

- Rated Impedance	: 16Ω

- HF Power re:AES2-2012	: 40W

- Waveguide Type	: square

- Nominal Coverage (HxV)	: 100°x10°

Power

- System Continuous Power	: HF:40W/LF:120W

- System Programme Power	: HF:80W/LF:240W

- System Peak Power	: HF:160W/LF:480W

- Crossover frequency	: 3.7kHz

Hardware

- Input Connector	: 2xSpeakon

Enclosure

- Cabinet type	: Trapezoid

- Enclosure Material and finish	: 15mm,18mm plywood

- Grille Material & Finish	: Steel

Dimensions (HxWxD)	: 536 x 363 x 164 mm

Net Weight	: 13 kg

* WLA-25 동급이상품.