외부안테나 분배기

1. 사  양

- Covering frequency	: 450 ~ 950MHz

- Low noise and amplifying circuit design

- Antenna Input / Output Impedance	: 50Ω

- Including Antenna cables for receiver connection x 8 pcs

- Including DC power cables for receiver connection x 4 pcs

- Including 3m BNC cables for external antenna connection x 2 pcs

- BNC connector

- Gain	: 3dB

- Power	: DC12V/3A Adapter

- Dimensions(mm)	: 448(W) x 44(H) x 160(D)

- Weight(g)	: 200g

◎ MAD908 및 동등 이상품