Sub speaker

1. 사  양

- FREQ.RESPONSE	:±6dB 35Hz 110KHz

- Axial Sensitivity(SPL,1W@1m)	: 98dB

- Impedance	: 4ohms

- Power handling	: 1000W(AES/RMS)/4000W(PEAK)

- Calculated Maximum(SPL@1m)	:Full range MAX 134dB

Full range long term 128dB

- Powering	: SUB Bass +1-1

- LF Subsystem	: 18" inch LF Driver 125MM Voice coil

- Enclosure Materials	: Plywood

- Finish/color	:Water resistant / Dark black coat

- Connectors	: 2xNL4 speakon

- Hardware	:ML-series integrated rigging

- Grille	: Powder coated perforated steel

- Filter	: Black Ester Foam

- Dimensions(WxHxD)	: 520 x 900 x 813MM

- Net weight	: 66.3kg

◎ ML118s 및 동등 이상품