Speaker

1. 기  능

본 기기는 6.5인치로 구성된 2way 스피커로서, 높은 명료도와 자연스러운 사운드를 얻을 수 있어야 한다.깨끗한 보컬 주파수 특성, 낮은 레벨에서 높은 레벨까지 왜곡이 없고, 음질 변화 없이 재생할 수 있어야 한다. 생음악, 음악 재생 및 연설을 포함하여 다양한 공간에서 적절하다.

2. 사  양

- Frequency Response(1W@1m)

±3dB	: 100Hz~20KHz

-10dB	: 90Hz~22KHz

- Axial Sensitivity(dB SPL,1W@1m): 91

- Impedance(Ohms)	: 8

- Power Handling  PROG(Watts) : Full Range 200

- Calculated Maximum Output(dB SPL@1m)

Full Range peak	: 119

Full Range Long Term	: 113

- Nominal Coverage Angle/-6dB points(Degrees)

Horizontal	: 90

Vertical	: 90

- System configuration	: Two-way full range

- Powering	: Passive(LF/HF crossover)

- LF subsystem	: 6.5" Woofer ×1

- HF subsystem	: 1"Thrpat HF(protection circuit)

- Enclosure Materials	: High intensity MDF Plywood

- Finish/color	: Water resistant textured/Black or White

- Connectors	: Speakon Binding Post Terminals

- Hardware

Top/Bottom	: Suspend Point×2

Rear	: Suspend Point×2

- Grille	: Power coated perforated steel
- Weight	: Net. 4.3Kg  (Gross  5.3Kg)

- Dimensions(W×H×D)	: 7.8""×12.2"×6.1"(198mm×310mm×155mm)

◎ MSR0610 및 동등 이상품