Speaker

1. 기  능

본 기기는 15인치로 구성된 2way 스피커로서, 높은 명료도와 자연스러운 사운드를 얻을 수 있어야 한다. 18mm 합판과 인클로저로 되어 깨끗한 보컬 주파수 특성, 낮은 레벨에서 높은 레벨까지 왜곡이 없고, 음질 변화 없이 재생할 수 있어야 한다. 생음악, 음악 재생 및 연설을 포함하여 다양한 공간에서 적절하다.

2. 사  양

- Frequency Response(1W@1m)

±3dB	: 60Hz~20KHz

-10dB	: 50Hz~22KHz

- Axial Sensitivity(dB SPL,1W@1m) : 99

- Impedance(Ohms)	: 8

- Power Handling RMS.PROGRAM/PEAK(Watts) : 400/800/1600

- Calculated Maximum Output(dB SPL@1m)

Full Range peak	: 124

Full Range Long Term	: 118

- Nominal Coverage Angle/-6dB points(Degrees)

Horizontal	: 90

Vertical	: 70

- System configuration	: Two-way full range

- Powering	: Passive(LF/HF crossover)

LF subsystem	: 15" Woofer ×1

HF subsystem	: 1.7"HF system protection circuit

- Enclosure Materials	: High intensity 18mm wood

- Finish/color	: Water resistant textured black point

- Connectors	: NL4 Speakon×2

- Hardware

Top/Bottom	: SPK Stand Pole Socket

Rear	: Suspend Point×2

Right/Left	: Suspend Point×2

- Grille	: Power coated perforated steel, foam backed

- Weight

Net.	: 21.3kg

Gross	: 26kg

- Dimensions(W×H×D)	: 16.9"×25.6"×15.4"(430mm×650mm×390mm)

◎ MSR1510 및 동등 이상품