품 명		FIXED I/O BOX
모 델		DL16	제조사	MIDAS
Technical Specifications
	16 award-winning MIDAS PRO microphone preamplifi ers with switchable +48 V phantom power 8 electronically balanced low impedance line level outputs ULTRANET personal monitoring system connectivity for in-ear applications Dual ADAT* outputs for use in splitter mode and stand-alone digital multicore applications Dual AES50 ports for cascading DL16 units—no merger or router required Remote operation up to 100 m via CAT5/5e cable All settings programmable from front panel controls or console Status indicator LEDs on front panel Headphones output assignable to any of the inputs or outputs for on-stage monitoring MIDI In/Out for bidirectional communication between FOH console and on-stage MIDI devices Features Neutrik etherCON* AES50 and ULTRANET network ports Rugged 2U rackmount chassis for durability in portable applications Auto-ranging universal switch-mode power supply Input : 16 ch Output : 8 ch AES50 : A,B ULTRANET : 1ch MIDI : In,Out Dim : 19" 2U

*) FIXED I/O BOX

1. 개요

본 기기는 Main Digital Mixer와 연동하여 사용가능한 Stage Box이다.

2. 기능 및 특성

16 award-winning MIDAS PRO microphone preamplifi ers with switchable +48 V phantom power

8 electronically balanced low impedance line level outputs

ULTRANET personal monitoring system connectivity for in-ear applications

Dual ADAT* outputs for use in splitter mode and stand-alone digital multicore applications

Dual AES50 ports for cascading DL16 units—no merger or router required

Remote operation up to 100 m via CAT5/5e cable

All settings programmable from front panel controls or console

Status indicator LEDs on front panel Headphones output assignable to any of the inputs or outputs for on-stage monitoring

MIDI In/Out for bidirectional communication between FOH console and on-stage MIDI devices

Features Neutrik etherCON* AES50 and ULTRANET network ports

Rugged 2U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Input	: 16 ch

Output	: 8 ch

AES50	: A,B

ULTRANET	: 1ch

MIDI	: In,Out

Dim	: 19" 2U

* DL16 동등이상품.