품 명		DIGITAL AUDIO MIXING CONSOLE
모 델		M 32R	제조사	MIDAS
Technical Specifications
	Live performance and studio recording digital console with up to 40 simultaneous input channels 16 award-winning MIDAS PRO microphone preamplifi ers 25 time-aligned and phase-coherent mix buses AES50 networking allows up to 96 inputs and 96 outputs Open architecture allows for future 96 kHz operation 192 kHz ADC and DAC converters for outstanding audio performance Industry-leading design by Bentley* Motors Designer High-performance aluminium and high-impact steel structure Rack mount brackets included for ultimate fl exibility 40 bit fl oating point digital signal processing 8 DCA and 6 mute groups 8 digital signal processing eff ects engines 17 MIDAS PRO motorised 100 mm faders Daylight viewable 5" full colour TFT display screen 32 x 32 channel USB 2.0 audio interface DAW remote control emulations of Mackie Control* and HUI* protocols Optional wireless remote control with MIDAS Apps for iPhone* and iPad* Main Screen : 5" TFT LCD, 800 x 480 Resolution, 262k Colours Channel LCD Screen : 128 x 64 LCD with RGB Colour Backlight Power Switch-Mode Power Supply : Auto-Ranging 100-240 VAC (50/60 Hz) Power Consumption : 70 W Physical Standard Operating Temperature Range : 5°C – 40°C (41°F – 104°F) Dimensions (W x H x D) : 478 x 617 x 208 mm Weight : 14.3 kg

(주)사운드솔루션

*) DIGITAL AUDIO MIXING CONSOLE

1. 개요

본 기기는 디지털 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Live performance and studio recording digital console with up to 40 simultaneous input channels

16 award-winning MIDAS PRO microphone preamplifi ers

25 time-aligned and phase-coherent mix buses

AES50 networking allows up to 96 inputs and 96 outputs

Open architecture allows for future 96 kHz operation

192 kHz ADC and DAC converters for outstanding audio performance

Industry-leading design by Bentley* Motors Designer

High-performance aluminium and high-impact steel structure

Rack mount brackets included for ultimate fl exibility

40 bit fl oating point digital signal processing

8 DCA and 6 mute groups

8 digital signal processing eff ects engines

17 MIDAS PRO motorised 100 mm faders

Daylight viewable 5" full colour TFT display screen

32 x 32 channel USB 2.0 audio interface

DAW remote control emulations of Mackie Control* and HUI* protocols

Optional wireless remote control with MIDAS Apps for iPhone* and iPad*

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Processing

Input Processing Channels	: 32 Input Channels, 8 Aux Channels, 8	FX Return Channels

Output Processing Channels	: 8 / 16

16 aux buses, 6 matrices, main LRC	: 100

Internal Effects Engines (True Stereo / Mono)

: 8 / 16

Internal Show Automation (structured Cues / Snippets)

: 500 / 100

Internal Total Recall Scenes (incl. Preamplifiers and Faders)

: 100

Signal Processing	: 40-Bit Floating Point

A/D Conversion (8-channel, 96 kHz ready)	: 24-Bit, 114 dB Dynamic Range,	A-weighted

D/A Conversion (stereo, 96 kHz ready)	: 24-Bit, 120 dB Dynamic Range,	A-weighted

I/O Latency (Console Input to Output)	: 0.8 ms

Network Latency (Stage Box In > Console > Stage Box Out)	: 1.1 ms

Connectors

MIDAS PRO Series Microphone Preamplifier (XLR)	: 16

Talkback Microphone Input (XLR)	: 1

RCA Inputs / Outputs	: 2 / 2

XLR Outputs	: 8

Monitoring Outputs (XLR / ¼"TRS Balanced)	: 2/2

Aux Inputs/Outputs (¼" TRS Balanced)	: 6 / 6

Phones Output (¼" TRS)	: 1 (Stereo)

AES50 Ports (KLARK TEKNIK SuperMAC)	: 2

Expansion Card Interface	: 32 Channel Audio Input / Output

ULTRANET P-16 Connector (No Power Supplied)

: 1

MIDI Inputs / Outputs	: 1 / 1

USB Type A(Audio and Data Import/Export)	: 1

USB Type B, rear panel, for remote control	: 1

Ethernet, RJ45, rear panel, for remote control

: 1

Mic Input Characteristics

Design	: MIDAS PRO Series

THD+N (0 dB gain, 0 dBu output)	: < 0.01% unweighted

THD+N (+40 dB gain, 0 dBu to +20 dBu output)

: < 0.03% unweighted

Input Impedance (Unbalanced / Balanced)	: 10 kΩ / 10 kΩ

Non-Clip Maximum Input Level	: +23 dBu

Phantom Power (Switchable per Input)	: +48 V

Equivalent Input Noise @ +45 dB gain (150 Ω source)	: -125 dBu 22 Hz-22 kHz, unweighted

CMRR @ Unity Gain (Typical)	: > 70 dB

CMRR @ 40 dB Gain (Typical)	: > 90 dB

Input/Output Characteristics

Frequency Response@48 kHz Sample Rate	: 0 dB to -1 dB 20 Hz – 20 kHz

Dynamic Range, Analogue In to Analogue Out

: 106 dB 22 Hz - 22 kHz, unweighted

A/D Dynamic Range, Preamplifier and Converter (Typical)

: 109 dB 22 Hz - 22 kHz, unweighted

D/A Dynamic Range, Converter and Output (Typical)

: 109 dB 22 Hz - 22 kHz, unweighted

Crosstalk Rejection @ 1 kHz, Adjacent Channels

: 100 dB

Output level, XLR Connectors (Nominal / Maximum)

: +4 dBu / +21 dBu

Output Impedance, XLR Connectors (Unbalanced / Balanced)

: 50 Ω / 50 Ω

Input impedance, TRS Connectors (Unbalanced / Balanced)

: 20 kΩ / 40 kΩ

Non-Clip Maximum Input Level, TRS Connectors

: +21 dBu

Output Level, TRS (Nominal / Maximum)	: +4 dBu / +21 dBu

Output Impedance, TRS (Unbalanced / Balanced)

: 50 Ω / 50 Ω

Phones Output Impedance / Maximum output Level

: 40 Ω / +21 dBu (Stereo)

Residual Noise Level, Out 1-16 XLR Connectors, Unity Gain

: -85 dBu 22 Hz-22 kHz, unweighted

Residual Noise Level, Out 1-16 XLR Connectors, Muted

: -88 dBu 22 Hz-22 kHz, unweighted

Residual Noise Level, TRS and Monitor out XLR Connectors

: -83 dBu 22 Hz-22 kHz, unweighted

Display

Main Screen	: 5" TFT LCD, 800 x 480 Resolution,	262k Colours

Channel LCD Screen	: 128 x 64 LCD with RGB Colour	Backlight

Main Meter	: 18 Segment (-45 dB to Clip)

Power

Switch-Mode Power Supply	: Auto-Ranging 100-240 VAC (50/60 Hz)	± 10%

Power Consumption	: 70 W

Physical

Standard Operating Temperature Range	: 5°C – 40°C (41°F – 104°F)

Dimensions	: 478 x 617 x 208 mm

Weight	: 14.3 kg

* M 32R 동등이상품.

DIGITAL AUDIO MIXING CONSOLE

1. 개요

본 기기는 디지털 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Live performance and studio recording digital console with up to 40 simultaneous input channels

16 award-winning MIDAS PRO microphone preamplifi ers

25 time-aligned and phase-coherent mix buses

AES50 networking allows up to 96 inputs and 96 outputs

Open architecture allows for future 96 kHz operation

192 kHz ADC and DAC converters for outstanding audio performance

Industry-leading design by Bentley* Motors Designer

High-performance aluminium and high-impact steel structure

Rack mount brackets included for ultimate fl exibility

40 bit fl oating point digital signal processing

8 DCA and 6 mute groups

8 digital signal processing eff ects engines

17 MIDAS PRO motorised 100 mm faders

Daylight viewable 5" full colour TFT display screen

32 x 32 channel USB 2.0 audio interface

DAW remote control emulations of Mackie Control* and HUI* protocols

Optional wireless remote control with MIDAS Apps for iPhone* and iPad*

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

XLR 입/출력	: 16 / 8ch

Signal Processing	: 40-Bit Floating Point

A/D Conversion (8ch, 96kHz ready) : 24-Bit, 114 dB Dynamic Range, A-weighted

D/A Conversion (ST, 96kHz ready)	: 24-Bit, 120 dB Dynamic Range, A-weighted

I/O Latency (Console In to Out)	: 0.8 ms

Network Latency (Stage Box In > Console > Stage Box Out)	: 1.1 ms

Connectors

- Microphone Preamplifier	: (XLR) 16

- Talkback Microphone Input	: (XLR) 1

- RCA Inputs / Outputs	: 2 / 2

- XLR Outputs	: 8

- Monitoring Outputs	: (XLR, 1/4" TRS Balanced) 2 / 2

- Aux Inputs/Outputs	: (1/4" TRS Balanced) 6 / 6

- Phones Output	: (1/4" TRS) 1(Stereo)

- Expansion Card Interface	: 32 Channel Audio Input/Output

- AES50 Ports (KLARK TEKNIK SuperMAC) x 2

- ULTRANET P-16 Connector (No Power Supplied) x 1

- MIDI Inputs x 1

- MIDI Outputs x 1

- USB Type A(Audio and Data Import/Export) x 1

- USB Type B, rear panel, for remote control x 1

- Ethernet, RJ45, rear panel, for remote control x 1

Main Screen	: 5" TFT LCD, 800x480 Resolution, 262k Colours

Channel LCD Screen	: 128 x 64 LCD with RGB Colour Backlight

Main Meter	: 18 Segment (-45 dB to Clip)

Switch-Mode Power Supply	: Auto-Ranging 100-240 VAC (50/60 Hz) ± 10%

Power Consumption	: 70 W

Standard Operating Temperature Range

: 5°C ~ 40°C

Dimensions	: 478 x 617 x 208 mm

Weight	: 14.3 kg

* M 32R 동등이상품.