품 명		SUBWOOFER SPEAKER
모 델		WLA-25SUB	제조사	Wharfedale
Technical Specifications
	System Type : Passive Frequency Response (+/-3dB) : 56Hz-1.5kHz Frequency Range (-10dB) : 56Hz-2.0kHz Calculated Maximum SPL @1m : 141dB System Rate Impedance : 4Ω Low Frequency Transducer - Size (mm / inches) : 254mm / 10" - Coil Size (mm / inches) : 65.5mm / 2.5" - LF Magnet Material : ferrite - LF Frame Material : aluminium - Rated Impedance : 8Ω - LF Power re:AES2-2012 : 2x350W Power - System Continuous Power : 700W - System Programme Power : 1400W - System Peak Power : 2800W Dimensions (HxWxD) : 536 x 400 x 550 mm Net Weight : 37 kg

*) SUBWOOFER SPEAKER

1. 개요

본 기기는 메인 스피커와 라인어레이 형태로 설치 가능한 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

700W RMS/1400W Program/2800W Peak power handling

Road tough modular subwoofer system

Dual 10" woofer, 2.5" voice coil

Nominal Impedance 4 Ohm

Strong internal bracing prevents bass loss and distortion from enclosure, vibration and resonance

2xParallel Speakon Inputs

3. 규격 및 사양

System Type	: Passive

Configuration	: Subwoofer

Frequency Response (+/-3dB)	: 56Hz-1.5kHz

Frequency Range (-10 dB)	: 56Hz-2.0kHz

Sensitivity (2.83v/1m)	: 107dB

Calculated Maximum SPL @1m	: 141dB

System Rated Impedance	: 4Ω

Low Frequency Transducer

- LF Size	: 254mm / 10"

- LF Voice-Coil Size	: 65.5mm / 2.5"

- LF Magnet Material	: ferrite

- LF Frame Material	: aluminium

- Rated Impedance	: 8Ω

- LF Power re:AES2-2012	: 2x350W

Power

- System Continuous Power	: 700W

- System Programme Power	: 1400W

- System Peak Power	: 2800W

Hardware

- Input Connector	: 2xSpeakon

Enclosure

- Cabinet type	: square

- Enclosure Material and finish	: 15mm,18mm plywood

- Grille Material & Finish	: Steel

Dimensions (HxWxD)	: 536 x 400 x 550 mm

Net Weight	: 37 kg

* WLA-25SUB 동급이상품.