Line Array

1. 사  양

- Frequence Reseponse	: ±6dB 65Hz~18KHz

- Axial Sensitivity(SPL,1W@1m)	: 97dB

- Impedance	: 8ohm

- Power handling	: 300W(AES/RMS) / 1200W(PEAK)

- Calculated Maximum(SPL@1m)	: Full range peak 127.5dB

Full range long term 121.5dB

- Nominal Coverage Angle / -6dB point(degrees): H90° / V 10°

- System Configuration	: 2way full range

- Powering	: Passive or bi-amplified(crossover built in)

: Full range +1-1

- LF Subsystem	: 1 x 10” inch LF Driver 75.5mm Voice coil

- HF Subsystem	: 1”throut DUAL 34mm HF driver,system protection circuit

- Enclosure Materials	: Plywood

- Finish / color	: Water resistant / Dark black coating

- Connectors	: 2 x NL4 speakon

- Hardware	: ML-series integrated rigging

- Grille	: Power coated perforated steel

- Filter	: Black Ester Foam

- Dimensions (H×W×D)	: 520 × 315 × 407mm

- Weight	: 20 kg

◎ ML110 및 동등 이상품