Speaker

1. 사  양

- Performance

- Frequency Response(1W@1m)	: ±3dB 100Hz~26KHz

: -10dB 60Hz~28KHz

- Axial sensitivity SPL,1W@1m(dB)	: Full Range 89

- Impedance(Ohms)	: Full Range 8

- Power Handling Program/peak(Watts)	: Full Range 100/200

- Calculated Max Output(dB SPL @1m)	: Full Range peak 113

: FullRange Long term 107

- Nominal CoverageAngle	: Horizontal 90

/-6dB points(Degrees)	: Vertical 90

Physical

- System configuration	: Two-way full range

- Powering	: Passive

- LF subsystem	: 5.25" Woofer x1

- HF subsystem	: 0.5"HF(system protection circuit)

- Enclosure Materials	: ABS/Black

- Connectors	: Binding post

- Transformer -Volt	: 100V/7.5W,15W Selectable

- Hardware	: Wall mount bracket

- Weight	: Net.2kg(gross 3kg)

- Dimension	: W(184mm)xH(245mm)xD169mm

◎ MS50T 및 동등 이상품