Speaker

1. 사  양

- Frequency. Response(-3dB)	: 30Hz - 120Hz

- Sensitivity(1W@1m)	: 96 dB

- Maximum SPL @ 1m	: 121 dB

- LF subsystem	: 1 X 18"

- HF subsystem	: -

- Impedance	: 8 ohm

- Power rating (RMS/PROG/PEAK)	: 500/1000/2000W

- Dispersion (H X V)	: -

- Connectors	: 2 X NL4 Speakon

- Adjust	: Bypass Crossover / Crossover (120Hz)

- Dimensions mm (W X H X D)	: 510 X 650 X 490

- Weight	: 34.06 kg

◎ MSR18sub 및 동등 이상품