Speaker

1. 사  양

- Type / Drivers	: 2way/1 x 10” + 1”

- Nor.inputpower AES/Cont.	: 300/600W

- Max.recommended.Amplifier	: 350W

- SPL.Peak	: 128dB @ 1meter

- Frequency range	: 57Hz-20kHz

- Coverage With DHF	: 90°x60°

- Impedance	: 8Ω

- Crossover frequencies	: 3.5 kHz

- Dimension(W x H x D)	: 322 x 495 x 310mm

- Weight	: 13kg

◎ Natural10.1 및 동등 이상품