품 명		PASSIVE PA SPEAKER
모 델		DELTA X10	제조사	Wharfedale
Technical Specifications
	System Type : Passive Frequency Response (+/-3dB) : 65Hz-20kHz Frequency Range (-10dB) : 60Hz-20kHz Sensitivity (2.83v/1m) : 97dB Calculated Maximum SPL @1m : 128dB System Rated Impedance : 8Ω Low Frequency Transducer - Size : 288mm / 10" Paper - Voice Coil Size : 63.5mm / 2.5" - Rated Impedance : 8Ω High Frequency Transducer - HF Driver Type : Compression Driver - Voice Coil Size : 44.5mm / 1.75" Titanium - Exit Size : 25.4mm / 1" - Rated Impedance : 8Ω - Nominal Coverage (HxV) : 90° x 60° Power - System Power (Cont./Prg./Peak) : 300W / 600W / 1200W Dimensions (H x W-Front / W-Rear x D) : 500 x 338/212.4 x 330 mm Weight : 16.58 kg

*) PASSIVE PA SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 라우드 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

High power, low distortion cast frame woofers

1" exit, 1.75" titanium diaphragm compression drivers

Externally switchable full range/bi-amp operation

90°x60° elliptical waveguides

Dual angle pole mount receptacles

Plywood construction with internal bracing

4-way high impact plastic carry handles

Rhino Rock texturised composite finish

Parallel speakon compatible inputs

3. 규격 및 사양

System Type	: Passive

Configuration	: Two-way

Frequency Response (+/-3dB)	: 65Hz-20kHz

Frequency Range (- 10dB)	: 60Hz-20kHz

Sensitivity (2.83v/1m)	: 97dB

Calculated Maximum SPL @1m	: 128dB

System Rated Impedance	: 8Ω

Low Frequency Transducer

- Size	: 288mm / 10" Paper

- Voice Coil Size	: 63.5mm / 2.5"

- Rated Impedance	: 8Ω

- LF Power	: 300W

High Frequency Transducer

- HF Driver Type	: Compression Driver

- Voice Coil Size	: 44.5mm / 1.75" Titanium

- Exit Size	: 25.4mm / 1"

- Diaphragm Material	: Titanium

- Rated Impedance	: 8Ω

- HF Power	: 40W

- Nominal Coverage (HxV)	: 90° x 60°

Power

- System Continuous Power	: 300W

- System Programme Power	: 600W

- System Peak Power	: 1200W

- Crossover frequency	: 2.8kHz

- Input Connector	: 2 x NL4 (speakON Compatible)

Hardware

- Pole Mount	: Dual Angle (0° / 10° ) 35mm Socket

- Handles	: 2 on Sides

- Rigging points	: 9 x M10

- Enclosure Material	: 15mm Plywood

- Grille Material	: 1.5 mm Steel

Dimensions (H x W-Front / W-Rear x D) : 500 x 338/212.4 x 330 mm

Weight	: 16.58 kg

* DELTA X10 동급이상품.