Speaker

1. 사  양

- Type / Drivers	: 2way/1 x 12” + 1”

- Nom. Input Power AES/Cont.(W)	: 350/700W

- Max.recommended.Amplifier	: 400 W

- SPL. Peak	: 124 dB @ 1meter

- Frequency Range	: 65 Hz – 15kHz

- Coverage with DHF	: 60° x 60°

- Impedance	: 8 Ω

- Crossover Frequencies	: 2kHz

- Dimension(W x H x D)	: 370 x 550 x 350 mm

- Weight	: 17 Kg

◎ Cope12.1 및 동등 이상품