Speaker

1. 사  양

- Type / Drivers	: 2way/1 x 12” + 1”

- Nor.inputpower AES/Cont.	: 400/800W

- Max.recommended.Amplifier	: 450W

- SPL.Peak	: 132dB @ 1meter

- Frequency range	: 54Hz-20kHz

- Coverage With DHF	: 90°x60°

- Impedance	: 8Ω

- Crossover frequencies	: 2.5 kHz

- Dimension(W x H x D)	: 380 x 588 x 405mm

- Weight	: 16kg

◎ Natural12.1 및 동등 이상품