Speaker

1. 사  양

- Type / Drivers	: 2way/1 x 15” + 1”

- Nor.inputpower AES/Cont.	: 600/1,200W

- Max.recommended.Amplifier	: 650W

- SPL.Peak	: 133dB @ 1meter

- Frequency range	: 47Hz-20kHz

- Coverage With DHF	: 90°x60°

- Impedance	: 8Ω

- Crossover frequencies	: 3 kHz

- Dimension(W x H x D)	: 460 x 700 x 475mm

- Weight	: 21kg

◎ Natural15.1 및 동등 이상품