품 명		SUBWOOFER SPEAKER
모 델		DELTA X18B	제조사	Wharfedale
Technical Specifications
	System Type : Passive Frequency Response (+/-3dB) : 38Hz-1.5kHz(BI-AMP) Frequency Range (-10dB) : 30Hz-1.5kHz Sensitivity (2.83v/1m) : 99dB Calculated Maximum SPL @1m : 134dB System Rated Impedance : 8Ω or 4Ω Low Frequency Transducer - Size : 470mm / 18" - Voice Coil Size : 102mm / 4" - Rated Impedance : 8Ω or 4Ω Power - System Power (Cont./Prg./Peak) : 800W / 1600W / 3200W Dimensions (HxWxD) : 539 x 539 x 650 mm Weight : 37.3 kg

*) SUBWOOFER SPEAKER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

18" LF driver

4" voice coil

Birch plywood construction

Premium Rhino Rock paint

2 carry handles

3. 규격 및 사양

System Type	: Passive

Configuration	: Subwoofer

Frequency Response (+/-3dB)	: 38Hz-1.5kHz(BI-AMP)

Frequency Range (-10 dB)	: 30Hz-1.5kHz

Sensitivity (2.83v/1m)	: 99dB

Calculated Maximum SPL @1m	: 134dB

System Rated Impedance	: 8Ω or 4Ω

Low Frequency Transducer

- Size	: 470mm / 18"

- Voice Coil Size	: 102mm / 4"

- Rated Impedance	: 8Ω or 4Ω

- LF Power	(re:AES2-2012)	: 800W

Power

- System Continuous Power	: 800W

- System Programme Power	: 1600W

- System Peak Power	: 3200W

- Input Connector	: 2 x NL4 (speakON Compatible)

Hardware

- Pole Mount	: 35mm

- Handles	: 2 on Sides

- Enclosure Material	: 15mm Plywood

- Grille Material	: 1.5 mm Steel

Dimensions (HxWxD)	: 539 x 539 x 650 mm

Weight	: 37.3 kg

* DELTA X18B 동급이상품.