Speaker

1. 사  양

- Type / Drivers	: 2way/12",1"

- Frequency Range	: 65 Hz - 18kHz

- Coverage with DHF	: 90°x60°

- Power Rating(AES)	: 400W

- System Sensitivity(1W/1M)	: 99dB

- SPL(Cont./Peak)	: 126dB/129dB

- Impedance	: 8Ω

- Crossover frequencies	: 2 kHz

- Dimension(W x H x D)	: 390 x 580 x 420mm

- Weight	: 16kg

◎ CDV12.1 및 동등 이상품