Speaker

1. 사  양

- Type / Drivers	: 2way/1 x 15” + 1”

- Nor.inputpower AES/Cont	: 400/600W

- Max.recommended.Amplifier	: 450W

- SPL.Peak	: 129dB @ 1meter

- Frequency range	: 60Hz-20kHz

- Coverage With DHF	: 90°x60°

- Impedance	: 8Ω

- Crossover frequencies	: 3kHz

- Dimension(W x H x D)	: 460 x 640 x 420mm

- Weight	: 24kg

◎ Cope15.1 V4 및 동등 이상품