Line Array Speaker

1. 사  양

- Type / Drivers	: 1 x 12” subwoofer

- Nor.inputpower AES/Cont.	: 900/1,300W

- Max.recommended.Amplifier	: 900W

- SPL.Peak	: 132dB @ 1meter

- Frequency range	: 40Hz-500Hz

- Coverage With DHF	: -

- Impedance(Low/High)	: 8Ω

- Crossover frequencies	: 200Hz

- Dimension(W x H x D)	: 555 x 370 x 420mm

- Weight	: 17.5kg

◎ Cubic12sub 및 동등 이상품